Leveling Abstract

Third Order differential leveling were run through the benchmarks listed below prior to beginning data collection and prior to removal of the water level gauge. Results follow:

|  |  |
| --- | --- |
|  |  |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Station** | **Name** | |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | | **PBM** |  |  |  |  |  |  |  | | **Other BMs** | **PID** | **Station Datum (Ft)** | **Install**  **Elevation** | **Removal**  **Elevation** | **Delta** |
| **9418723** | **Fields Landing** | P 1087 |  | LV0263 | 30.354 | 30.35 | 30.35 | 0.00 |
|  |  |  | Q 1087 | LV0264 |  | 26.96 | 26.96 | 0.00 |
|  |  |  | 8723 TIDAL 7 RESET | LV0655 |  | 5.13 | 5.13 | 0.00 |
|  |  |  | 8739 C TIDAL | LV0652 |  | 4.02 | 4.02 | 0.00 |
|  |  |  | 8739 B TIDAL | LVO653 |  | 3.40 | 3.39 | -0.01 |

Station name: FIELD’S LANDING

Station number: 9418723

Instrument: LEICA NA3000, DNA 03, NA2

Rod type: STANDARD three-piece bar-code

Serial numbers: 90966, 539680

Date: Varies

Personnel: PARTY CHIEF, CHAINPERSON